# ProSoft MNET-61850 Configuration Manager 2.0.2.43 Read Me

ProSoft MNET-61850 Configuration Manager 2.0.2.43
ReadMe File

This ReadMe file contains information you should know before you install ProSoft MNET-61850 Configuration Manager version 2.0.2.43 This file also contains information that may not be available in other ProSoft Technology documentation. Visit our website for the most current information about ProSoft MNET-61850 Configuration Manager.

Version 2.0.2.43 Changes:

1. Fixes the reverse MNET Tags mapping issue.
2. Fixes the CID file crashing any version of PSW-MNET-61850 CM issue.
3. Fixed issue where Configuration Manager creates a corrupted project file when switching protocols on ports and attempting to download.
4. Fixed issue where Configuration Manager where it allows a project to be downloaded without a proper CID file confirmed path.

# ProSoft MNET-61850 Configuration Manager Compatibility

The following system requirements apply to ProSoft MNET-61850 Configuration Manager.

ProSoft MNET-61850 Configuration Manager installation instructions are provided in the ProLinx PLX8x-MNET-61850 user manual.

> Note: System requirements in this document are subject to change and do not represent a commitment to support any particular software or hardware.

## ProSoft MNET-61850 Configuration Manager Operating Systems Tested

- Windows 7 Professional (32-bit and 64-bit versions), 8 GB RAM Intel® Core™ i7 3770 (3.40 GHz)
- Windows 8 Professional (64-bit version), 8 GB RAM Intel® Core™ i7 3770 CPU(3.40 GHz)
- Windows 10 Professional (64-bit version), 32 GB RAM Intel® Core™ i7 6700 CPU(3.40 GHz)
- Windows 11 Professional (64-bit version), 32 GB RAM AMD Ryzen 5 5600H CPU(3.30 GHz)

> NOTE: To use ProSoft MNET-61850 Configuration Manager under the Windows 7 OS, you must be sure to install ProSoft MNET-61850 Configuration Manager using the Run as Administrator option. To find this option, right-click on the Setup.exe installer program icon. In the context menu, you will see the Run as Administrator option. Left-click to use this install option. Be aware, you must install using this option even if you are already logged in as an Administrator on your network or personal computer (PC). Using the Run as Administrator option will allow the ProSoft 61850 Configuration Manager installer to create folders and files on your PC with proper permissions and security. If you do not use the Run as Administrator option, ProSoft MNET-61850 Configuration Manager may appear to install correctly; but you will receive numerous, repeating file access errors whenever ProSoft MNET-61850 Configuration Manager is running, especially when changing configuration screens. If this happens, to eliminate the errors, you will have to completely uninstall ProSoft MNET-61850 Configuration Manager and then re-install using the Run as Administrator option.

# Previously Released version of ProSoft MNET-61850 Configuration Manager 2.0.2.37

Version 2.0.2.37 Changes:

1. Fixes issue on Optimize MNET Command mappings parameter not saving on .prj file.
2. Fixes issue on MNET Server mapping in reverse order from what was configured.

Version 2.0.2.30 Change:

1. Fixes issue with MMS not able to write.

Version 2.0.2.19 Change:

1. When the user attempts to download a project that is missing the Modbus TCP/IP bubble in the configuration file, the message box will pop up stating: This project is incomplete in that it is missing the ‘Modbus TCP/IP device’ and should not be downloaded.

Version 2.0.2.4 Changes:

1. Added the option to automatically group multiple tags as a single Function 16; PLX write to Modbus clients, making data transfer more effective.
2. Updated selection for PLX82 1-port functionality.
3. Updated Starting Read and Write ordinals in Generic Client property dialog.

Version 2.0.1.6 Changes:

1. Allow selection of ctlVal controllable element
2. Allows editing of M340 address fields
3. Fixes issue with M340 default addressing
4. Fixes issue where Multiple tags are associated with a single MNET Command.

Version 2.0.0.1 Changes:

1. Change tool name from ProSoft 61850 Configuration Manager to ProSoft MNET-61850 Configuration Manager
2. Report RptEnabled Max parameter set as 1 now adds 01 suffix
3. Resolves issue with GOOSE.indXX where XX>9
4. Resolves the Control Type Issue with PLX82
5. Restricts the database tag character limit to 50
6. Updates to the .SCL parser with regards to reports

ProSoft 61850 Configuration Manager 1.2.1.4

Detailed Reason(s) for Version 1.2.1.4 Changes:

1. Added support for Array type tags for controller
2. Fixed issue related to supporting up to 45 EIDS

ProSoft 61850 Configuration Manager 1.1.0.4

Detailed Reason(s) for Version 1.1.0.4 Changes:

1. Supports "rptEnabled" flag as used in Schneider CID files
2. Support for "Grouped" and "Ungrouped" Goose reports
3. Increased the IED connection limit to 45
4. Adjusts the MMSPath displayed in the app to be 61850 Spec compliant - ie: Adds domain name and Logical Device
5. Upper limit on GOOSE attributes has been bumped from 60 to 120
6. Fixes issue with the importing of Siemens CID files, changes to the PrjFiles
7. Fixes an issue with the mapping layout when using Auto-Assign tags and issue with "undo" button
8. Overall improvement of tag functionality and support of reports greater than 500 bytes
9. Allow the user to change the path where the project CID files are located

ProSoft 61850 Configuration Manager 1.0.9.17

Detailed Reason(s) for Version 1.0.9.17 Changes:

Added Modbus Mapping fot TCP/IP Client and Server.

ProSoft 61850 Configuration Manager 1.0.7.1

Detailed Reason(s) for Version 1.0.7.1 Changes:

Fixes uploading issue where the configuration file was uploaded using a new computer.

ProSoft 61850 Configuration Manager 1.0.4.7

Detailed Reason(s) for Version 1.0.4.7 Changes:

Supports SBO and enhanced security control, fixes compatibility issues with Areva CID files.

ProSoft 61850 Configuration Manager 1.0.0.96

Detailed Reason(s) for Version 1.0.0.96 Changes:

Initial Release.